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version：GV-M32SAP-GGS20170428

Shanghai Goodview Electronics Technology Co. Ltd.
32 inch Commercial LCD Monitor SPEC
Model：M32SAP
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Product Specifications
	Display

	Panel
	31.55 inches LED backlight(LD320DUE-FHB1)

	Active Area(mm)
	698.4（H）×392.9(V）

	Aspect Ratio
	16:9

	Resolution
	1920×1080

	Brightness
	400 cd/m2

	Contrast Ratio
	1100：1

	Viewing Angle
	178°

	Display Colors
	16.7M

	Life Expectancy
	50000 hours

	System configuration 

	CPU
	Dual-cores ARM Cortex A9 1.5 GHz（max 1.6GHz）

	GPU
	Four cores ARM Mali-400 MP

	Memory 
	1GB

	Storage 
	8GB

	Operating system 
	Android 4.2

	Touch

	Touch type
	/

	Touch point
	/

	Touch precision
	/

	Response time
	/

	External ports

	Signal ports
	VGA*1、HDMI*1、AUDIO*1

	Network ports
	LAN（RJ45）

	Storage extension
	32G

	Other ports
	USB2.0*2

	Multimedia

	media file formats
	video：MMPEG1、MPEG2、MPEG4、H.264、WMV、MKV、TS、flv

	
	audio: MP3 、WMA、 M4A、AAC

	
	picture: PG、JPEG、BMP、PNG、GIF

	
	text：txt

	Play mode
	Horizontal screen, Vertical screen, full screen and split screen play

	Program transmission mode
	USB、LAN、Wan

	Machine parameters

	Product size (mm)
	723.4（H）×422.9（V）×68（D）

	Carton size（mm）
	813.4（H）×510（V）×163.4（D）

	Installation mode
	Horizontal hanging、Vertical hanging

	VESA（mm）
	400*200

	Screen suspension mode
	landscape、portrait

	Menu language
	Chinese、English

	Machine color
	black

	Weight 
	net：9.8KG  gross：12.1KG

	Power consumption
	42W

	Speaker 
	Stereo 4Ω2W*2

	Watchdog function
	support

	Timing 
	Multi-time timing power on/off, port timing automatic switch

	Management software
	Ezposter/GTV

	Power supply
	AC100-240V(50/60HZ)

	Working Temp.（°C）
	0〜40℃

	Working Humidity（RH）
	10% 〜 80%RH

	Storage environment
	Temperature: - 10 ~ 60 ℃ / humidity: 10% ~ 90% RH

	Accessories
	Product warranty card 1, remote control * 1, certificate * 1, quick start guide * 1, power line * 1, safety and environmental protection considerations * 1, WIFI antenna * 1, M&PF series hang nail sleeve * 4, M8 * 40 bolt * 4

	Certificates
	CCC/CECP


Schematic Drawing
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Product Images
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Packaging
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