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Shanghai Goodview Electronics Technology Co. Ltd.
55 inch Commercial LCD Monitor SPEC
Model：M55SAP
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Product Specifications
	Display

	Panel
	54.64 inches LED backlight/modelLD550EUE-FHB1

	Active Area(mm)
	1209.6（H）×680.4(V）

	Aspect Ratio
	16:9

	Resolution
	1920×1080

	Brightness
	450 cd/m2

	Contrast Ratio
	1100:1

	Viewing Angle
	178°

	Display Colors
	16.7M

	Life Expectancy
	50000 hours

	System configuration 

	CPU
	Dual-cores ARM Cortex A9 1.5 GHz（max 1.6GHz）

	GPU
	Four cores ARM Mali-400 MP

	Memory 
	1GB

	Storage 
	8GB

	Operating system 
	Android 4.2

	Touch

	Touch type
	/

	Touch point
	/

	Touch precision
	/

	Response time
	/

	External ports

	Signal ports
	VGA*1、HDMI*1、AUDIO*1

	Network ports
	LAN（RJ45）

	Storage extension
	32G

	Other ports
	USB2.0*2

	Multimedia

	media file formats
	video：MMPEG1、MPEG2、MPEG4、H.264、WMV、MKV、TS、flv

	
	audio: MP3 、WMA、 M4A、AAC

	
	picture: PG、JPEG、BMP、PNG、GIF

	
	text：txt

	Play mode
	Horizontal screen, Vertical screen, full screen and split screen play

	Program transmission mode
	USB、LAN、Wan

	Machine parameters

	Product size (mm)
	1232（H）×708.9（V）×59.3（D）

	Carton size（mm）
	1361（H）×825.4（V）×193.7（D）

	Installation mode
	Horizontal hanging、Vertical hanging

	Screen suspension mode
	landscape、portrait

	Menu language
	Chinese、English

	Machine color
	black

	Weight 
	net：29.6KG  gross：36.5KG

	Power consumption
	68W

	Speaker 
	Stereo 4Ω2W*2

	Watchdog function
	support

	Timing 
	Multi-time timing power on/off, port timing automatic switch

	Management software
	Ezposter/GTV

	Power supply
	AC100-240V(50/60HZ)

	Working Temp.（°C）
	0~ 40℃

	Working Humidity（RH）
	10% ~ 80%RH

	Storage environment
	Temperature: - 10 ~ 60 ℃ / humidity: 10% ~ 90% RH

	Accessories
	Product warranty card * 1, remote control * 1, qualified certificate * 1, quick start guide * 1, power line * 1, safety and environmental protection precautions * 1, WIFI antenna * 1

	Certificates
	CCC 
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Packaging 
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