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Shanghai Goodview Electronics Technology Co. Ltd.

32-inch LCD Monitor

Model:M32SC 
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Product Specifications
	Display

	Panel
	31.5 inches LED backlight 

	Active Area(mm)
	715.0（H）×411.0（V）

	Aspect Ratio
	16:9

	Resolution
	1366×768 

	Brightness
	240-330 cd/m2

	Contrast Ratio
	1200:1

	Viewing Angle
	( R/L 89 (Min.), U/D 89 (Min.))

	Display Colors
	8bit, 16.7 Million

	Color temperature
	10000K

	Life Expectancy
	30000 hours

	Response time
	8ms

	System configuration                                     

	Main board
	MSD6A338-T8C1 

	Operating system
	Android 4.4

	CPU
	Double-cores ARM Cortex A17 structure/（1.2GHz）,

	GPU
	Four cores ARMMail-764

	Memory 
	1GB DD3

	Storage 
	8G eMMc    

	External ports

	Signal ports
	HDMI×3、Audio out（3.5mm）×1、AV Inx1

	Network ports
	LAN*1（10/100MEthernet） 

	Storage extension
	USB flash disk  128G (Max)

	Other ports
	   USB（2.0）×2  

	Multimedia

	media file formats
Play mode
	video：Support MPEG1, MPEG2, MPEG4, H.264, WMV, MKV, TS, FLV and other mainstream video format

	
	audio：Support MP3 and other audio formats

	
	picture：Support JPG, JPEG, BMP, PNG, GIF, etc

	
	text：/

	
	Other: interactive playback

	Play mode
	Horizontal screen, full screen and split screen 

	Program transmission mode
	USB、LAN、WAN

	Machine parameters

	Product size (mm)
	730 (H)×430(V)×75(D)

	Carton size（mm）
	855（H）×542（V）×132（D）

	VESA（mm）
	100×100

	Screen suspension mode
	landscape

	Menu language
	Chinese、English

	Machine color
	black

	Weight 
	net：3.5KG
	gross：5KG

	Power consumption
	55W (Max)

	Speaker 
	stereo 2×2W 4Ω

	intelligent volume
	/   

	Watchdog function
	/

	Timing 
	Multi-time timing power on/off（Electricity and networking are valid）

	Management software
	Signway Cloud Management system

	Power supply
	AC~100-240V (50/60Hz)

	Working Humidity（RH）
	  5℃〜40℃   10% 〜 85%RH  No condensation

	Storage environment
	-20℃〜55℃   5% 〜 75%RH  No condensation

	Accessories
	warranty card ×1
remote control×1

	Certificates
	CCC/CECP


Schematic Drawing
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Product Images
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Packaging
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