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Shanghai Goodview Electronics Technology Co. Ltd.

49 inch Commercial LCD Monitor SPEC
Model：M49SDP
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Product Specifications
	Display

	Panel
	48.50 inches LED backlight(LD490EUE-FHB1)

	Active Area(mm)
	1073.78（H）×604(V）

	Aspect Ratio
	16:9

	Resolution
	1920×1080

	Brightness
	450 cd/m2

	Contrast Ratio
	1100:1

	Viewing Angle
	178°

	Display Colors
	16.7M

	Life Expectancy
	30000 hours

	System configuration 

	CPU
	/

	GPU
	MST6E182VG

	Memory 
	/

	Storage 
	/

	Operating system 
	/

	Touch

	Touch type
	/

	Touch point
	/

	Touch precision
	/

	Response time
	/

	External ports

	Signal ports
	VGA*1、HDMI*1、AUDIO*1

	Network ports
	/

	Storage extension
	/

	Other ports
	USB2.0*1、RS232(DB9)*1

	Multimedia

	media file formats
	video：MMPEG1、MPEG2、MPEG4、H.264、WMV、MKV、TS、flv

	
	audio: MP3 、WMA、 M4A、AAC

	
	picture: PG、JPEG、BMP、PNG、GIF

	
	text：txt

	Play mode
	Full screen round robin

	Program transmission mode
	USB 

	Machine parameters

	Product size (mm)
	1096.16（H）×632.5（V）×59.3（D）

	Carton size（mm）
	1225.16（H）×749（V）×193.7（D）

	Installation mode
	Horizontal hanging、Vertical hanging

	Screen suspension mode
	landscape、portrait

	Menu language
	Chinese、English

	Machine color
	black

	Weight 
	net：25.3KG  gross：29.2KG

	Power consumption
	53W

	Speaker 
	Stereo 4Ω2W*2

	Watchdog function
	/

	Timing 
	Multi-time timing power on/off

	Management software
	/

	Power supply
	AC100-240V(50/60HZ)

	Working Temp.（°C）
	0〜40℃

	Working Humidity（RH）
	10% 〜 80%RH

	Storage environment
	Temperature: - 10 ~ 60 ℃ / humidity: 10% ~ 90% RH

	Accessories
	Product warranty card 1, remote control * 1, certificate * 1, quick start guide * 1, power line * 1, safety and environmental protection considerations * 1, VGA line * 1

	Certificates
	CCC 


Schematic Drawing
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Packaging 
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