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Shanghai Goodview Electronics Technology Co. Ltd.


70 inch Commercial LCD Monitor
Model:M70STL
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Product Specifications
	Display

	Panel
	69.5 inches LED backlight  

	Active Area (mm) 
	865.6（H）×1538.9（V）

	Aspect Ratio
	16:9

	Resolution 
	3840×2160 

	Brightness
	320 cd/m2

	Contrast Ratio 
	3200:1

	Viewing Angle (CR>10) 
	All view angle ( R/L 156 (Min.), U/D 156 (Min.))

	Display Colors 
	10bit, 1.07 Billion

	Color temperature 
	TBD

	Back light bulb Life
	30000 hours

	Response time 
	8ms

	System configuration                      

	Operating system
	Android 5.0.1

	CPU
	ARM A53×4 1.4GHz

	GPU
	ARM Mali450 MP4(4+2) 450MHz

	Memory 
	2G

	Storage 
	16G 

	Touch                                   

	Touch type
	Infrared touch

	Touch Points
	20 points 

	Interpolation resolution
	32767×32767

	Touch accuracy
	 ±2mm(More than 90% of the touch area)

	Response time
	<15ms

	Enter mode
	Finger, stylus, opaque objects

	Smallest touch objects
	Single
	6mm

	
	Multipoint 
	8mm

	External ports

	Signal ports
	HDMI(1.3) IN×2
VGA IN×1
VGA Audio IN×1
DP IN×1
AV ×1
YPBPR×1
AV OUT×1
Audio OUT×1

	Network ports
	Wired network: LAN×1（RJ45 10/100M Ethernet） 
wireless network:  WiFi×1（802.11bgn）

	Storage extension
	Micro SD Card ×1  

	Other ports
	AC Switch×1 
AC IN×1
USB 3.0 IN×2
Touch OUT USB（TypeB）×1  
IR IN×1 (3.5mm JACK)
RS232×1 (DB9) 
SPDIF×1

	Multimedia   

	picture
	File extension name
	*.jpg, *.bmp, *.png

	
	The encoder
	Standard RGB

	
	Maximum image resolution
	Baseline : 
JPG : 6000 x 6000
GIF : 1920 x 1080
BMP : 1920 x 1080
PNG : 1920 x 1

	
	Maximum filename length
	128 bytes

	video
	File extension name
	*.mpg, *.avi, *.mp4, *.mkv, *flv, *.mov, , *.ts, 

	
	Coding and code rate
	MPEG-1        bitrate<20Mbps  
MPEG-2        bitrate<40Mbps
MPEG-4        bitrate<30Mbps
H.264            bitrate<30Mbps
AVC              bitrate<30Mbps
H263           bitrate<30Mbps
XVID         bitrate<30Mbps

	audio
	File extension name
	*.mp3,AAC, wav

	
	The encoder
	MPEG Audio, PCM

	text
	File extension name
	*.txt

	
	Encoder format
	ANSI、

	Play mode
	Horizontal screen, Vertical screen, full screen and split screen play

	Program transmission mode
	USB、LAN、Wan

	Other parameters

	Product size  (mm)
	959.25(H)×1633.10(V)×112.80(D)

	Package  size（mm）
	1255（H）×1810（V）×345（D）

	VESA（mm）
	400×600 & 400×400 （Screw type M8×25mm）

	Screen hanging mode
	landscape、portrait

	Menu language
	Chinese、English

	Machine color
	black

	Weight
	net：50KG (TBD)
	gross：64KG (TBD)

	Power Consumption
	205W (Max)

	Speaker 
	stereo 2×10W 8Ω

	Smart volume
	time-sharing volume

	Watchdog 
	N/A 

	Timing function
	Multi-time timing power on/off, port timing automatic switch

	Management software
	GTV Information Distribution System

	Power supply
	AC~100-240V (50/60Hz  3 Hz )  

	Working environment 
	  0〜40℃   10% 〜 85%RH  No condensation

	Storage environment
	-10〜60℃   10% 〜 75%RH  No condensation

	Accessories
	1. Warranty card * 1.
2. Certificate of qualification
3. Quick start guide x 1.
4. AC power line x 1 (national standard)
5. 2.4G WiFi antenna x 1 root.
6. Remote control * 1.
7. AAA battery x 2Pcs.
8.Safety and environmental considerations *1

	Certificates
	CCC/FCC
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