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Shanghai Goodview Electronics Technology Co. Ltd.
55 inch Commercial LCD Monitor SPEC
Model：M55SAP
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Product Specifications
	Display

	Panel
	54.64 inches LED backlight（LD550EUE-FHB1）

	Active Area(mm)
	1209.6（H）×680.4(V）

	Aspect Ratio
	16:9

	Resolution
	1920×1080 

	Brightness
	450 cd/m2

	Contrast Ratio
	1100:1

	Viewing Angle
	 ( R/L 89 (Min.), U/D 89 (Min.))

	Display Colors
	8bit, 16.7 Million

	Life Expectancy
	10000K

	Panel
	50000 hours

	Active Area(mm)
	12ms

	System configuration                                      

	Operating system 
	Android 4.2

	CPU
	Dual-cores ARM Cortex A9 1.5 GHz（max 1.6GHz）

	GPU
	Four cores ARM Mali-400 MP

	Memory 
	DDR3 1Gbyte

	Storage 
	NAND FLASH 8GB

	External ports

	Signal ports
	VGA×1、HDMI×1、VGA Audio IN×1

	Network ports
	LAN*1（10/100M）、WIFI(802.11bgn)

	Storage extension
	Micro TF Card×1  32G (Max)

	Other ports
	USB2.0×2、SIM Card×1、DC Switch×1

	Multimedia

	media file formats
	video：MMPEG1、MPEG2、MPEG4、H.264、WMV、MKV、TS、flv

	
	audio: MP3 、WMA、 M4A、AAC

	
	picture: PG、JPEG、BMP、PNG、GIF

	
	text：txt

	Play mode
	Horizontal screen, Vertical screen, full screen and split screen play

	Program transmission mode
	USB、LAN、Wan

	media file formats
	video：MMPEG1、MPEG2、MPEG4、H.264、WMV、MKV、TS、flv

	Machine parameters

	Product size  (mm)
	1232（H）×708.9（V）×59.3（D）

	Package size（mm）
	1377（H）×825.4（V）×209（D）

	VESA（mm）
	400*400

	Screen hanging mode
	Landscape、Portrait

	Menu language
	Chinese、English

	Machine color
	black

	Weight 
	Net：30.9KG  
	Weight：38.5KG

	Power Consumption
	68W  (Max)

	Speaker 
	stereo 2×2W 4Ω

	Smart volume
	time-sharing volume

	Watchdog timer
	support

	Timing function
	Multi-time timing power on/off, port timing automatic switch

	Management software
	C/S framework: ADPE/Ezposter  

B/S framework: GTV Information Distribution System

	Power supply
	AC~100-240V (50/60Hz)

	Working environment 
	  0〜40℃   10% 〜 85%RH  No condensation

	Storage environment
	-10〜60℃   10% 〜 90%RH  No condensation

	Accessories
	1. Power line x 1

2. Remote control

3. AAA battery x 2

4. Certificate of conformity x 1

5. Product warranty card x 1

6. Quick start guide x 1

7. Safety and environmental protection considerations x 1

8. WIFI antenna x 1

9. M&PF series hook sleeve x 4

10. M8 x 40 boltsx 4



	Certificates
	CCC/CECP
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Product Images 
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Packaging
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