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49-inch Multi-media LCD Digital Signage 

Model:M49STP
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Product Specifications
	Display

	Panel
	48.5 inches LED backlight(model: LD490EUE-FHB1）

	Active Area(mm)
	1073.78（H）×604（V）

	Aspect Ratio
	16:9

	Resolution
	1920×1080 

	Brightness
	450 cd/m2

	Contrast Ratio
	1100:1

	Viewing Angle
	 ( R/L 89 (Min.), U/D 89 (Min.))

	Display Colors
	8bit, 16.7 Million

	Color temperature
	10000K

	Life Expectancy
	50000 hours

	Response time
	12ms

	System configuration                                      

	Main-board  scheme
	SWH5180 

	Operating system
	Android 5.1

	CPU
	4 core ARM Cortex A17 （max 1.8GHz）,

	GPU
	4 core ARMMail-764

	Memory 
	2GB 

	Storage 
	8G eMMC

	Touch                                    

	Touch device model
	FB49WH00D-CT-A1

	Touch type
	Infrared touch

	Touch point
	10 points

	Touch resolution
	32767×32767

	Touch precision
	±2mm(more than 90% of the touch area)

	Response time
	<15ms

	Input mode
	Finger, touch pen and other opaque objects

	Minimum touch object
	Single point
	5ms

	
	Multi-point
	8ms

	External ports

	Signal ports
	HDMI IN×1、VGA IN×1、VGA Audio IN×1

	Network ports
	LAN(10/100M)×1 、WiFi×1(802.11bgn)、3/4 Mobile network (optional)

	Storage extension
	TF Card×1 （Max 32G）

	Other ports
	AC IN×1、AC Switch×1、USB（Android）×2 、Touch USB OUT×1、
IR IN（3.5mm）×1

	Multimedia

	media file formats
	video： MPEG1、MPEG2、MPEG4、H.264、WMV、MKV、TS、flv 

	
	audio：Support MP3 and other mainstream audio formats

	
	picture： JPG、JPEG、BMP、PNG、GIF 

	
	text：txt

	
	other： none

	Play mode
	Horizontal screen, portrait screen, full screen and split screen play

	Program transmission mode
	USB、LAN、Wan

	Machine parameters

	Product size (mm)
	1134.2(H)×665.2(V)×73.1(D) 

	Carton size（mm）
	1303（H）×830（V）×265（D）

	VESA (mm)
	300×400

	Screen suspension mode
	Landscape、Portrait

	Menu language
	Chinese、English

	Machine color
	black

	Weight 
	net：39.6 KG
	net：39.6 KG

	Power consumption
	95W (Max)

	Speaker 
	stereo 2×2W 4Ω

	intelligent volume
	time-sharing volume/adaptive volume

	watchdog function
	Support 

	Timing 
	Multi-time timing power on/off, port timing automatic switch

	Management software
	C/S framework: ADPE/Ezposter  

B/S framework: GTV Information Distribution System

	Power supply
	AC~100-240V (50/60Hz)

	Working Humidity（RH）
	  0〜40℃   10% 〜 85%RH  No condensation

	Storage environment
	-10〜60℃   10% 〜 90%RH  No condensation

	Accessories
	AC power cord * 1 （National standard）

remote control * 1
AAA battery * 2
2.4G WiFi antenna * 1
USB line* 1
Safety and environmental protection considerations * 1
certificate * 1
warranty card * 1

	Certificates
	CCC/CECP
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Product Images 
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Packaging
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