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Shanghai Goodview Electronics Technology Co. Ltd.

43-inch LCD multimedia Touch Table
Model: PF43H8C2

Revision History
	Part number
	version
	Revise Date
	Prepared by
	Checked by
	approval
	Remarks

	1380078
	GV- PF43H8C2-GGS20170216
	2017\6\13
	[image: image1.png]



	[image: image2.png]



	[image: image3.png]



	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


Note：All right reserved by Goodview.Please contact with us for the latest updates.
Product Specification
	Display Panel

	Panel 

	42.51 inches LED backlight （LD550EUE-FHB1）

	Active Area(mm)
	941.184（H）×529.416（V）

	Aspect Ratio
	16：9

	Resolution
	1920×1080

	Brightness
	450 cd/m2

	Contrast Ratio
	1100:1

	Viewing Angle
	 ( R/L 89 (Min.), U/D 89 (Min.))

	Color 
	8bit, 16.7 Million

	Color temperature
	10000K

	Backlight lamp life
	50000 hours

	Response time
	12ms

	System                                       

	Main board model
	SWH3188

	CPU
	/

	GPU 
	/,

	Memory 
	/

	Storage 
	/

	Operation system
	/

	Touch                                  

	Model 
	WGJ430008A-QDA-A1

	Touch type
	Capacitive touch

	Touch Points
	10 points

	Interpolation resolution
	16384*9600（MAX）

	Touch accuracy
	 ±1mm (More than 90% of the touch area)

	Response time
	<20ms

	Enter mode
	Skin type conductors

	Smallest touch objects
	Single 
	/

	
	Multi-point
	/

	ports

	Signal port
	HDMIx1、VGAx1、Audio IN×1

	Network ports
	\

	Storage extension
	\

	Other 
	AC Switch×1  \   USB（2.0）×1  \  USB Touch×1

IR IN（3.5mm JACK）×1  RS232（DB9 JACK）×1

	multimedia

	Media file formats
	video：AVC/HEVC (H.264) video decoding up to 1080p60 

	
	audio：MP3

	
	picture：JPEG、BMP、PNG

	
	text：txt

	
	Other: support interactive play 

	Play mode
	\

	Program transmission way
	\

	Other parameters 

	Product Size(mm)
	1360(H)×703(V)×870(D)

	Package Size(mm）
	1472*815*1092

	VESA（mm）
	/

	Screen hanging mode
	/

	Menu language
	Chinese, English 

	Machine color
	White + wood grain

	Weight 
	net：50KG
	gross：60KG

	Power Consumption
	51W (Max)

	Speaker
	stereo 2×2W 8Ω

	Watchdog timer
	/          

	Smart volume
	/

	Timing function
	multiple time periods programmable power on/off

	Management software
	/

	Power supply
	AC~100-240V (50/60Hz)

	Working environment
	  0〜40℃   10% 〜 85%RH  No condensation

	Storage environment
	-10〜60℃   10% 〜 90%RH  No condensation

	Accessories
	1. AC power cord x 1 (US standard)

2.HDMI line x1
3.Remote controlx 1



	Certificates
	/


Schematic Drawing
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Product Images
[image: image5.jpg]


[image: image6.jpg]


[image: image7.png]


[image: image8.png]


[image: image9.jpg]|
/3
SR
Wy
%‘ﬂ’ —
P
.

—
=

RIN IR TOUCH USB RS232 AUDIO VGA HDMI USB AC SWITCH AC IN




[image: image10.jpg]80.00

1360.00

941.20(B=Xid,

0008 _ _

(XA d5) 2y 625
00°€0L

00048




Packaging
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